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The following paper for scientific students competition road nr.82– a second rated highroad between Veszprém and Győr - will be inspected from a road safety point of view.
The steps of the inspection are below presented:
- introduction of the applied methodology
- preparation of the inspection
- going over the highroad
- creating the inspection the database
- investigating black spots on the investigated road section
- completing the database
- evaluation of the recorded data.
introduction of the inspection method: testing the operation method of the assessing equipments, introduction of the main definitions.
preparation for the inspection: setting up the measuring system, (laptop, cameras, and GPS).
going over the investigated road: recording the view of the road between Veszprém to Győr
creating the inspection database: collecting the proper aspects of the assessment .
investigating black spots on the investigated road section: assigning the black spot of the last 3 years
completing the database: road safety inspection of records belonging to the assigned accidents
evaluation of the recorded data: searching for correlation between accidents and the quality of road. Finally suggestions will be made about changing the road to avoid further accidents.




